{"text_format":"1","workbook":"xlsx","n_sheets":5,"sheets":["Size solar panel","DATA","Solar Insolation Map (World)","Solar Insolation Map (Africa)","1"],"not_rendered":{"charts":0,"images":2,"macros":1,"external_links":0,"defined_names":17,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Size solar panel","index":0,"n_rows":43,"n_cols":14,"rows_kept":43,"cut":false,"hidden":false,"merged":[[0,1,4,4],[0,5,1,11],[2,5,4,11],[5,1,9,4],[5,5,9,5],[5,6,9,6],[5,7,9,7],[5,8,9,8],[5,9,9,9],[5,10,9,10],[5,11,9,11],[12,1,13,11],[14,1,16,4],[14,5,16,5],[14,6,16,6],[14,7,16,7],[14,8,16,8],[14,9,16,9],[14,10,16,10],[14,11,16,11],[14,13,16,18],[29,9,34,11],[30,1,30,4],[31,1,31,4],[32,1,32,4],[33,1,33,4],[39,1,39,4],[39,6,39,7],[40,1,40,4],[40,6,40,7],[42,1,42,4]]}
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,1,1]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"^Veuillez saisir la quantité d’auxiliaires Centurion utilisés et le nombre d’utilisations \npar jour"]
[]
[]
[null,null,null,null,null,1,1]
[null,null,null,null,null,1,1]
[null,null,null,null,null,1,1]
[null,null,null,null,null,1,1]
[null,null,null,null,null,1,1]
[null,null,null,null,null,1,1]
[null,null,null,null,null,1,1]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,"Notes:"]
[null,"Puissance NETTE Requise:",null,null,null,null,0,"Wh"]
[null,"Détarage dû à la poussière, etc:",null,null,null,0.2,0,"Wh"]
[null,"Fournir une surcharge pour charger complètement la batterie:",null,null,null,0.15,0,"Wh"]
[null,"Insolation Géographique (heures/jour):",null,null,null,4.75,0,"W"]
[]
[]
[]
[]
[]
[null,"Autonomie:",null,null,null,1,"Jours"]
[null,"DoD Autorisée pour la batterie utilisée:",null,null,null,0.2,"Cycle profond de préférence"]
[]
[null,"Capacité Totale (Ah) Nécessaire : ",null,null,null,null,{"$error":"#N/A"},"Ah"]

{"sheet":"DATA","index":1,"n_rows":81,"n_cols":14,"rows_kept":81,"cut":false,"hidden":false,"merged":[[2,2,2,3],[2,5,2,6],[2,7,2,8],[40,2,40,3],[40,5,40,6],[40,7,40,8]]}
[]
[]
[null,"VOLTS","COURANT",null,"TEMPS","ÉNERGIE",null,"WATTS"]
["MOTEUR","TENSION DU SYSTÈME","COURANT DE REPOS (mA)","COURANT ACTIF (A)","TEMPS/FONCTIONNEMENT - Secondes Actives (OUVRIR ET FERMER, etc.)","Ah de repos consommé (par 24h)","Ah actif consommé (par cycle)","W de repos consommé (par 24h)","W actif consommé (par cycle)",null,"AUTOMATE","FACTEUR"]
["Moteur D2 Turbo pour Portails Coulissants ",12,95,8,20,{"$f":"IF(C5>0,C5/1000*24,\"\")","v":2.2800000000000002},{"$f":"IF(A5<>\"\",IF(D5>0,D5*E5/(60*60),C5),\"\")","v":4.4444444444444446E-2},{"$f":"IF(C5>0,F5*B5,\"\")","v":27.360000000000003},{"$f":"IF(D5>0,G5*H5,\"\")","v":1.2160000000000002},null,"Automate - D2 Turbo",1]
["Moteur D5-EVO pour Portails Coulissants ",12,75,8,30,{"$f":"IF(C6>0,C6/1000*24,\"\")","v":1.7999999999999998},{"$f":"IF(A6<>\"\",IF(D6>0,D6*E6/(60*60),C6),\"\")","v":6.6666666666666666E-2},{"$f":"IF(C6>0,F6*B6,\"\")","v":21.599999999999998},{"$f":"IF(D6>0,G6*H6,\"\")","v":1.44},null,"Automate - EVO",1]
["Moteur D10 pour Portails Coulissants  (système de 24V CC)",24,80,6,30,1.92,0.05,46.08,2.3039999999999998,null,"Automate - D10",0.65]
["Moteur D10 Turbo pour Portails Coulissants (système de 24V CC)",24,80,10,20,1.92,5.5555555555555552E-2,46.08,2.5599999999999996,null,"Automate - D10",0.65]
["Moteur A10 pour Portails Coulissants (utilisant un convertisseur CC)",12,16,20,30,0.38400000000000001,0.16666666666666666,4.6080000000000005,0.76800000000000002,null,"CP201",1]
["Moteur R3 pour Portails Battants Simples",12,16,4,35,0.38400000000000001,3.888888888888889E-2,4.6080000000000005,0.17920000000000003,null,"CP75",1]
["Moteur R3 pour Portails Battants Doubles",12,16,8,35,0.38400000000000001,7.7777777777777779E-2,4.6080000000000005,0.35840000000000005,null,"CP75",1]
["Moteur R5 pour Portails Battants Simples",12,16,5,40,0.38400000000000001,5.5555555555555552E-2,4.6080000000000005,0.25600000000000001,null,"CP75",1]
["Moteur R5 pour Portails Battants Doubles",12,16,10,40,0.38400000000000001,0.1111111111111111,4.6080000000000005,0.51200000000000001,null,"CP75",1]
["Moteur MAXI-MATE pour Portails Battants Simples",12,25,5,40,0.60000000000000009,5.5555555555555552E-2,7.2000000000000011,0.4,null,"CP77",1]
["Moteur MAXI-MATE pour Portails Battants Doubles",12,25,10,40,0.60000000000000009,0.1111111111111111,7.2000000000000011,0.8,null,"CP77",1]
["Moteur VECTOR pour Poratils Battants Simples (V400)",12,48,2,28,1.1520000000000001,1.5555555555555555E-2,13.824000000000002,0.21504000000000001,null,"Automate - SÉRIE V",1]
["Moteur VECTOR pour Poratils Battants Simples (V500)",12,48,2,35,1.1520000000000001,1.9444444444444445E-2,13.824000000000002,0.26880000000000004,null,"Automate - SÉRIE V",1]
["Moteur VECTOR pour Poratils Battants Doubles (V400)",12,48,4,28,1.1520000000000001,3.111111111111111E-2,13.824000000000002,0.43008000000000002,null,"Automate - SÉRIE V",1]
["Moteur VECTOR pour Poratils Battants Doubles (V500)",12,48,4,35,1.1520000000000001,3.888888888888889E-2,13.824000000000002,0.53760000000000008,null,"Automate - SÉRIE V",1]
["Moteur VANTAGE pour Portails Battants Simples (VT400)",12,73,2,28,1.7519999999999998,1.5555555555555555E-2,21.023999999999997,0.32703999999999994,null,"Automate - SÉRIE V",1]
["Moteur VANTAGE pour Portails Battants Simples (VT500)",12,48,2,35,1.1520000000000001,1.9444444444444445E-2,13.824000000000002,0.26880000000000004,null,"Automate - SÉRIE V",1]
["Moteur VANTAGE pour Portails Battants Doubles (VT400)",12,48,4,28,1.1520000000000001,3.111111111111111E-2,13.824000000000002,0.43008000000000002,null,"Automate - SÉRIE V",1]
["Moteur VANTAGE pour Portails Battants Doubles (VT500)",12,48,4,35,1.1520000000000001,3.888888888888889E-2,13.824000000000002,0.53760000000000008,null,"Automate - SÉRIE V",1]
["Moteur VERT-X pour Portails Battants Simples (VX300)",12,48,2,25,1.1520000000000001,1.3888888888888888E-2,13.824000000000002,0.192,null,"Automate - SÉRIE V",1]
["Moteur VERT-X pour Portails Battants Doubles (VX300)",12,48,4,32,1.1520000000000001,3.5555555555555556E-2,13.824000000000002,0.49152000000000007,null,"Automate - SÉRIE V",1]
["Barrière SECTOR (3M)",12,50,2,2.5,1.2000000000000002,1.3888888888888889E-3,14.400000000000002,2.0000000000000004E-2,null,"Automate - SECTOR",1]
["Barrière SECTOR (4.5M or 6.0M)",12,50,2,6,1.2000000000000002,3.3333333333333335E-3,14.400000000000002,4.8000000000000008E-2,null,"Automate - SECTOR",1]
["Moteur D5-EVO pour Portails Coulissants avec Extenseur d'Impulsions",12,75,8.1,30,1.7999999999999998,6.7500000000000004E-2,21.599999999999998,1.458,null,"Automate - EVO",1]
["Moteur D5 Smart pour Portails Coulissants (système de 24V CC)",24,60,8,25,1.44,5.5555555555555552E-2,34.56,1.92,null,"Automate - DX ",1,null,"Portail de 5 mètres à 32m/min, 2.5 sec de montée et descente"]
["Moteur D10 Smart pour Portails Coulissants (système de 24 VCC)",24,60,9,35,1.44,8.7499999999999994E-2,34.56,3.024,null,"Automate - DX ",1,null,"Portail de 6 mètres à 24m/min, 2.5 sec de montée et descente"]
["Moteur D10 Turbo Smart pour Portails Coulissants (système de 24 VCC)",24,60,10,20,1.44,5.5555555555555552E-2,34.56,1.92,null,"Automate - DX ",1,null,"Portail de 6 mètres à 42m/min, 2.5 sec de montée et descente"]
["Moteur D20 Smart pour Portails Coulissants (système de 24V CC)",24,60,10,40,1.44,0.1111111111111111,34.56,3.84,null,"Automate- DX ",1,null,"Portail de 6 mètres à 18m/min, 2.5 sec de montée et descente"]
["Moteur R6 pour Portails Battants Simples ",12,25,4,30,0.60000000000000009,3.3333333333333333E-2,7.2000000000000011,0.24000000000000002,null,"CP77",1]
["Moteur R6 pour Portails Battants Doubles ",12,25,8,30,0.60000000000000009,6.6666666666666666E-2,7.2000000000000011,0.48000000000000004,null,"CP77",1]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[]
[null,"VOLTS","COURANT",null,"TEMPS","ÉNERGIE",null,"WATTS"]
["ACCESSOIRES",{"$f":"+B4","v":"TENSION DU SYSTÈME"},{"$f":"+C4","v":"COURANT DE REPOS (mA)"},"COURANT ACTIF (A)","TEMPS/FONCTIONNEMENT - Secondes Actives (OUVRIR ET FERMER, etc.)","Ah de repos consommé (par 24h)","Ah actif consommé (par cycle)","W de repos consommé (par 24h)","W actif consommé (par cycle)"]
["Régulateur solaire de 20A (ESOLRPG020V1)",12,6,null,null,{"$f":"IF(C43>0,C43/1000*24,\"\")","v":0.14400000000000002},{"$f":"IF(A43<>\"\",IF(D43>0,D43*E43/(60*60),C43),\"\")","v":6},{"$f":"IF(C43>0,F43*B43,\"\")","v":1.7280000000000002},{"$f":"IF(D43>0,G43*H43,\"\")","v":""}]
["Faisceaux infrarouges I5 - Tx & Rx",12,67,null,null,{"$f":"IF(C44>0,C44/1000*24,\"\")","v":1.6080000000000001},{"$f":"IF(A44<>\"\",IF(D44>0,D44*E44/(60*60),C44),\"\")","v":67},{"$f":"IF(C44>0,F44*B44,\"\")","v":19.295999999999999},{"$f":"IF(D44>0,G44*H44,\"\")","v":""}]
["Faisceaux de Sécurité PHOTON",12,30,null,null,0.72,30,8.64,""]
["Récepteur CENTURION avec 1 canal",12,11,null,null,0.26400000000000001,11,3.1680000000000001,""]
["Récepteur CENTURION avec 4 canaux",12,25,0.18,0.5,0.60000000000000009,2.4999999999999998E-5,7.2000000000000011,1.8000000000000001E-4]
["Récepteur Supa Helix",12,100,0.27,0.5,2.4000000000000004,3.7500000000000003E-5,28.800000000000004,1.0800000000000002E-3]
["Le G-Switch 22",12,80,null,null,1.92,80,23.04,""]
["MYGSM 88",12,120,null,null,2.88,120,34.56,""]
["Panneau d'Entrée POLOphone ",12,35,null,null,0.84000000000000008,35,10.080000000000002,""]
["Combiné POLOphone ",12,25,null,null,0.60000000000000009,25,7.2000000000000011,""]
["G-Speak Classic (Plus)",12,30,null,null,0.72,30,8.64,""]
["Intercom Mkii GSM ",12,350,0.15,null,8.3999999999999986,0,100.79999999999998,0]
["SMARTGUARD (Câblé)",12,32,0.18,null,0.76800000000000002,0,9.2160000000000011,0]
["Lecteur SOLO",12,50,0.18,null,1.2000000000000002,0,14.400000000000002,0]
["Automate Lattice",12,50,0.18,null,1.2000000000000002,0,14.400000000000002,0]
["Lecteur Esclave Lattice",12,50,0.18,null,1.2000000000000002,0,14.400000000000002,0]
["Détecteur de Boucle Autonome FLUX",12,50,null,null,1.2000000000000002,50,14.400000000000002,""]
["Détecteur de Boucle Enfichable FLUX 11",12,50,null,null,1.2000000000000002,50,14.400000000000002,""]
["Convertisseur CC-CC (utilisé avec 10A pour la batterie de secours)",12,150,null,null,3.5999999999999996,150,43.199999999999996,""]
["Bord Sensible",12,30,null,null,0.72,30,8.64,""]
["Extenseur d'Impulsions",12,7,null,null,0.16800000000000001,7,2.016,""]
["G-ULTRA 2G",12,33,0.35,15,0.79200000000000004,1.4583333333333334E-3,9.5040000000000013,1.3860000000000003E-2]
["G-SPEAK ULTRA 2G",12,130,0.35,15,3.12,1.4583333333333334E-3,37.44,5.4599999999999996E-2]
["G-ULTRA 3G PENTA BAND",12,130,0.35,15,3.12,1.4583333333333334E-3,37.44,5.4599999999999996E-2]
["WiZo",12,30,null,null,0.72,30,8.64,""]
["Feux de Circulation",12,20,null,null,{"$f":"IF(C68>0,C68/1000*24,\"\")","v":0.48},20,{"$f":"IF(C68>0,F68*B68,\"\")","v":5.76},{"$f":"IF(D68>0,G68*H68,\"\")","v":""}]
["Automate des CLAWS",12,70,null,null,1.6800000000000002,70,20.160000000000004,""]
["Pas de Bouton-Poussoir Tactile",12,30,null,null,0.72,30,8.64,""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[null,null,null,null,null,"","","",""]
[]
["Tension du Système"]
[12]
[24]

{"sheet":"Solar Insolation Map (World)","index":2,"n_rows":37,"n_cols":2,"rows_kept":37,"cut":false,"hidden":false,"merged":[[24,0,24,1],[0,0,0,3]]}
["Carte d’Ensoleillement - Monde"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["FRANCE"]
["VILLE","Heures d’Ensoleillement Effectives"]
["RENNE",1.24]
["NANTES",1.46]
["LE HAVRE",1.18]
["BORDEAUX",1.81]
["TOULOUSE",2.5299999999999998]
["MARSEILLE",2.97]
["NICE",2.58]
["MONTPELLIER",1.65]
["LYON",1.56]
["REIMS",0.95]
["PARIS",1.1100000000000001]

{"sheet":"Solar Insolation Map (Africa)","index":3,"n_rows":72,"n_cols":8,"rows_kept":72,"cut":false,"hidden":false,"merged":[[0,0,0,3],[2,6,2,7]]}
["Carte d’Ensoleillement - Afrique"]
[]
[null,null,null,null,null,null,"Countries"]
[null,null,null,null,null,null,"English","French"]
[null,null,null,null,null,null,"Algeria ","Algérie"]
[null,null,null,null,null,null,"Angola","Angola"]
[null,null,null,null,null,null,"Benin","Bénin"]
[null,null,null,null,null,null,"Botswana","Botswana"]
[null,null,null,null,null,null,"Burkina Faso","Burkina Faso"]
[null,null,null,null,null,null,"Burundi","Burundi"]
[null,null,null,null,null,null,"Cabo Verde","Cap-Vert"]
[null,null,null,null,null,null,"Cameroon","Cameroun"]
[null,null,null,null,null,null,"Central African Republic","République Centrafricaine"]
[null,null,null,null,null,null,"Chad","Tchad"]
[null,null,null,null,null,null,"Comoros","Comores"]
[null,null,null,null,null,null,"Congo","Congo"]
[null,null,null,null,null,null,"Côte d’Ivoire","Côte d’Ivoire"]
[null,null,null,null,null,null,"Cyprus","Chypre"]
[null,null,null,null,null,null,"Democratic Republic of the Congo","République Démocratique du Congo"]
[null,null,null,null,null,null,"Djibouti","Djibouti"]
[null,null,null,null,null,null,"Egypt","Égypte"]
[null,null,null,null,null,null,"Equatorial Guinea","Guinée Équatoriale"]
[null,null,null,null,null,null,"Eritrea","Érythrée"]
[null,null,null,null,null,null,"Ethiopia","Éthiopie"]
[null,null,null,null,null,null,"Gabon","Gabon"]
[null,null,null,null,null,null,"Gambia","Gambie"]
[null,null,null,null,null,null,"Ghana","Ghana"]
[null,null,null,null,null,null,"Guinea","Guinée"]
[null,null,null,null,null,null,"Guinea-Bissau","Guinée-Bissau"]
[null,null,null,null,null,null,"Iran","Iran"]
[null,null,null,null,null,null,"Iraq","Irak"]
[null,null,null,null,null,null,"Israel","Israël"]
[null,null,null,null,null,null,"Jordan","Jordanie"]
[null,null,null,null,null,null,"Kenya","Kenya"]
[null,null,null,null,null,null,"Kuwait","Koweït"]
[null,null,null,null,null,null,"Lebanon","Liban"]
[null,null,null,null,null,null,"Lesotho","Lesotho"]
[null,null,null,null,null,null,"Liberia","Libéria"]
[null,null,null,null,null,null,"Libya","Libye"]
[null,null,null,null,null,null,"Madagascar","Madagascar"]
[null,null,null,null,null,null,"Malawi","Malawi"]
[null,null,null,null,null,null,"Mali","Mali"]
[null,null,null,null,null,null,"Malta","Malte"]
[null,null,null,null,null,null,"Mauritania","Mauritanie"]
[null,null,null,null,null,null,"Mauritius","Maurice"]
[null,null,null,null,null,null,"Morocco","Maroc"]
[null,null,null,null,null,null,"Mozambique","Mozambique"]
[null,null,null,null,null,null,"Namibia","Namibie"]
[null,null,null,null,null,null,"Niger","Niger"]
[null,null,null,null,null,null,"Nigeria","Nigéria"]
[null,null,null,null,null,null,"Oman","Oman"]
[null,null,null,null,null,null,"PNA","ANP"]
[null,null,null,null,null,null,"Qatar","Qatar"]
[null,null,null,null,null,null,"Rwanda","Rwanda"]
[null,null,null,null,null,null,"Sao Tome and Principe","Sao Tomé-et-Principe"]
[null,null,null,null,null,null,"Saudi Arabia","Arabie Saoudite"]
[null,null,null,null,null,null,"Senegal","Sénégal"]
[null,null,null,null,null,null,"Seychelles","Seychelles"]
[null,null,null,null,null,null,"Sierra Leone","Sierra Leone"]
[null,null,null,null,null,null,"Somalia","Somalie"]
[null,null,null,null,null,null,"South Africa","Afrique du Sud"]
[null,null,null,null,null,null,"Sudan","Soudan"]
[null,null,null,null,null,null,"Syria","Syrie"]
[null,null,null,null,null,null,"Tanzania","Tanzanie"]
[null,null,null,null,null,null,"Togo","Togo"]
[null,null,null,null,null,null,"Tunisia","Tunisie"]
[null,null,null,null,null,null,"Uganda","Ouganda"]
[null,null,null,null,null,null,"United Arab Emirates","Émirats Arabes Unis"]
[null,null,null,null,null,null,"West Sahara","Sahara Occidental"]
[null,null,null,null,null,null,"Yemen","Yémen"]
[null,null,null,null,null,null,"Zambia","Zambie"]
[null,null,null,null,null,null,"Zimbabwe","Zimbabwe"]

{"sheet":"1","index":4,"n_rows":1,"n_cols":1,"rows_kept":1,"cut":false,"hidden":true,"merged":[]}
["solar"]